{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["数据","sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"数据","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"sheet1","index":1,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,1,1,5],[1,6,1,9],[2,1,2,9],[3,1,3,4],[3,6,3,9],[7,2,7,3],[7,6,7,7],[8,2,8,3],[8,6,8,7],[9,2,9,3],[9,6,9,7],[10,2,10,3],[10,6,10,7],[11,2,11,3],[11,6,11,7],[12,2,12,3],[12,6,12,7],[13,2,13,3],[13,6,13,7],[14,2,14,3],[14,6,14,7],[15,2,15,3],[15,6,15,7],[16,2,16,3],[16,6,16,7],[17,2,17,3],[17,6,17,7],[18,2,18,3],[18,6,18,7],[19,2,19,3],[19,6,19,7],[20,2,20,3],[20,6,20,7],[21,2,21,3],[21,6,21,7],[22,2,22,3],[22,6,22,7],[23,2,23,3],[23,6,23,7],[24,2,24,3],[24,6,24,7],[25,0,25,1],[26,0,26,1],[27,0,27,1],[30,0,30,9],[31,1,31,2],[31,4,31,5],[31,6,31,7],[31,8,31,9],[32,0,32,9],[4,0,6,0],[4,1,6,1],[25,2,27,2],[28,2,29,2],[5,5,6,5],[4,2,6,3],[4,6,6,7],[28,0,29,1],[25,3,27,9],[28,3,29,9]]}
["防雷装置检测原始记录"]
["  编码：                                                                         ","J特Q3.01-2018-   ",{"$nulls":4},"     第    页"]
["委托单位： "]
[" 受检单位： ",{"$nulls":4},"检测地点："]
["分布区域","序号"," 装置部位名称",null,"接闪器","装置及连接状况\n","具体方位",null," 接地电","检测结论"]
[{"$nulls":4},"及状况","合格（○）\n其它\n",null,null," 阻值","合  格（○）"]
[{"$nulls":8},"（Ω）","不合格（×）"]
{"$rows_empty":18}
["依据标准：",null,"钳形接地电阻表： ","□12170 □12171 □12172 □12173 □11917 □11920 □11944"]
["□ GB50057-2010《建筑物防雷设计规范》"]
["□ GB15599-2009《石油与石油设施雷电安全规范》"]
["□ GB/T 21431-2015《建筑物防雷装置检测技术规范》",null,"接地电阻表：","□8212128 □8212130 □8212150 □8212148 □8212230  □8100809     □8100813\n"]
[]
["□一类防雷接地电阻标准值≤10Ω □二类防雷接地电阻标准值≤10Ω □三类防雷接地电阻标准值≤30Ω "]
["检测人：",null,null,"校核人：",null,null,"检测日期：  ",null,"2018年   月   日"]
["保存部门：宇信质量检测有限公司                                           保存期限：6年"]